From 3b5c462273686d7d479a988718a26468f0bc3ef5 Mon Sep 17 00:00:00 2001
From: Clifford Wolf <clifford@clifford.at>
Date: Wed, 5 Feb 2014 15:06:13 +0100
Subject: presentation progress

---
 manual/PRESENTATION_ExSyn.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/PRESENTATION_ExSyn.tex')

diff --git a/manual/PRESENTATION_ExSyn.tex b/manual/PRESENTATION_ExSyn.tex
index f183da93..9aa9bfeb 100644
--- a/manual/PRESENTATION_ExSyn.tex
+++ b/manual/PRESENTATION_ExSyn.tex
@@ -348,7 +348,7 @@ Finally the {\tt fsm\_map} command can be used to convert the (optimized) {\tt
 \begin{frame}[t]{\subsecname}
 \vbox to 0cm{\includegraphics[width=12cm,trim=-18cm 0cm 0cm -34cm]{PRESENTATION_ExSyn/techmap_01.pdf}\vss}
 \vskip-0.8cm
-The {\tt techmap} command replaces cells with an implementations given as
+The {\tt techmap} command replaces cells with implementations given as
 verilog source. For example implementing a 32 bit adder using 16 bit adders:
 
 \vbox to 0cm{
-- 
cgit v1.2.3

